1

1

2

2 3

4

4

5

5

6

6

7

7

8

8

A A

B B

C C

D D

          will be installed, but not both.

NOTE: C7 (tantalum) or C22 (electrolytic)

P3D-RUDAKU-V53-01 3.1

Power Control and Reset

Lyle Johnson, WA7GXD and the RUDAK Team.

Copyright (C) 1994, 1995,1996.

B 10 15

Friday, July 05, 1996

Title

Size Document Number Rev

Date: Sheet of

+10VA

+10VB

PWRCTL

+10V

+5V +10SW

VCC

GND VSS

C16 0.1 uF

U14 LM2576T-5.0

+VIN 1 FBK 4

+VOUT 2 ON/OFF 5 G N D 3

L3

680 uH

C36 0.1 uF

D1

MBR350 D2

MBR350

D5 MBR350

F1

FUSE

Q2 2N2222 C48 0.1 uF

C49 0.1 uF C19 0.1 uF C21 0.1 uF

C119 0.1 uF

C118 0.1 uF

C127 0.1 uF

C126 0.1 uF C31 0.1 uF C33 0.1 uF

F2

FUSE

R33

1K

L1

40 uH

C7 22 uF

+

C63 47 uF

+ C64

47 uF

+ C65 47 uF

+

C66 47 uF

+ C62

47 uF

+ C56 47 uF

+

R59 220 ohms

Q3 TIP125

Q1

IRF9530

C22 100 uF

+

R91 10K

+10VA

+10VB

PWRCTL